Assignment-2
1. Define stability factors S, S’, and S”. Draw the circuit diagram of a self-bias circuit and derive its stability factors S, S’, and S”.
2. A CE amplifier is drawn in by a voltage source of internal resistance RS = 800 Ω and load impedance RL = 1 KΩ . The h-parameters are hie = 1 KΩ , hre = 2X10-4, hfe = 50 and hoe = 25 µA/V. Compute AI, AV,RI and RO.
3. Differentiate between BJT and FET. Explain the construction and operation of an n-channel MOSFET.

